{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet0"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet0","index":0,"n_rows":42,"n_cols":4,"rows_kept":42,"flags":["formulas_cached_only"]}
["模块描述","分值","得分","原因"]
["串口服务器无线","2.00","2.00",""]
["工业网闸有线","3.00","0.00","属性：【dxgl】【dxgl】【clgl_rkwg】【clgl_rkip】【clgl_ckwg】【clgl_ckip】【clgl_wdyml】，正确值：【[{\"dx_name\":\"有线区交换机\",\"iplx\":\"IPV4\",\"ip\":\"192.168.66.4\"},{\"dx_name\":\"数采服务器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.60.7\"}]】【[{\"dx_name\":\"有线区交换机\",\"iplx\":\"IPV4\",\"ip\":\"192.168.66.4\"},{\"dx_name\":\"数采服务器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.60.7\"}]】【192.168.80.6】【192.168.36.4】【192.168.49.6】【192.168.49.5】【拒绝】，错误值：【[{\"dx_name\":\"数采服务器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.66.4\"},{\"dx_name\":\"有线区交换机\",\"iplx\":\"IPV4\",\"ip\":\"192.168.80.5\"}]】【[{\"dx_name\":\"数采服务器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.66.4\"},{\"dx_name\":\"有线区交换机\",\"iplx\":\"IPV4\",\"ip\":\"192.168.80.5\"}]】【】【】【】【】【允许】"]
["串口服务器有线","2.00","2.00",""]
["工业网闸无线","3.00","0.00","属性：【dxgl】【clgl_wdyml】，正确值：【[{\"dx_name\":\"无线区路由器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.131.8\"},{\"dx_name\":\"数采服务器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.60.7\"}]】【拒绝】，错误值：【[{\"dx_name\":\"无线区路由器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.132.6\"},{\"dx_name\":\"数采服务器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.60.7\"}]】【允许】"]
["云端配置页面网关维护","2.00","2.00",""]
["DB-IotLite网关有线","4.00","0.00","属性：【tdpz_watchtime】【mqtt_sssjfbzt】，正确值：【1】【dbzn/gateway/iotlite/2000808010】，错误值：【0】【dbzn/gateway/iotlite2000808010】"]
["DB-IotLite网关无线","3.00","0.00","属性：【ippz_wifi_ssid】【ippz_zwym】【tdpz_td】【tdpz_qdmc】【tdpz_chuankou】【tdpz_btl】【tdpz_sjw】【tdpz_tzw】【tdpz_jojy】【tdpz_watchtime】【sbpz_sbdz】【cjdpz_tagid】【cjdpz_mc】【cjdpz_jcqdz】【mqtt_qiyong】【mqtt_ip】【mqtt_port】【mqtt_wgsn】【mqtt_sssjfbzt】【mqtt_qos】【mqtt_scms】【mqtt_sczq】【DBIotLiteWx】【mqtt_cjd_sbmc】【mqtt_cjd_tagid】，正确值：【无线区无线网】【255.255.255.192】【串口】【ModbusRTU_over_TCP】【com1】【9600】【8】【1】【无校验（none）】【1】【1】【MachinePamHID909】【急停状态】【8193】【1】【192.168.60.7】【1883】【2000808012】【dbzn/gateway/iotlite/2000808012】【qos1】【周期上传】【5】【[\"采集成功\"]】【无线区精雕1】【MachinePamHID909】，错误值：【无线区无限网】【255.255.255.129】【网口】【ModbusTCPClient】【】【】【】【】【】【0】【192.168.160.5】【MachinePamHID910】【产量】【8195】【】【】【】【】【】【】【】【】【】【】【】"]
["斥候工业网关有线","3.00","0.00","属性：【sbpz_ip】【cjdpz_tagid】【cjdpz_mc】【cjdpz_jcqdz】【mqtt_sssjfbzt】【mqtt_cjd_tagid】，正确值：【192.168.96.3】【MachinePamHID917】【主轴转速】【8210】【dbzn/gateway/iotlite/2000808011】【MachinePamHID917】，错误值：【192.168.96.4】【MachinePamHID910】【产量】【8195】【dbzn/gateway/iotlite2000808011】【MachinePamHID910】"]
["云端配置页面网关配置","2.00","2.00",""]
["斥候工业网关无线","3.00","0.00","属性：【sbpz_ip】【sbpz_qyhmcj】【sbpz_qyplcj】【sbpz_zqsbonchange】【mqtt_sssjfbzt】，正确值：【192.168.129.5】【0】【1】【0】【dbzn/gateway/iotlite/2000808013】，错误值：【192.168.129.6】【false】【true】【false】【abzn/gateway/iotlite2000808013】"]
["串口服务器无线","2.00","2.00",""]
["云端配置页面网关配置","2.00","2.00",""]
["DB-IotLite网关有线","4.00","4.00",""]
["DB-IotLite网关无线","3.00","0.00","属性：【ippz_wifi_mm】【tdpz_cgsj】，正确值：【admin1234!】【1000】，错误值：【admin1234！】【100】"]
["串口服务器有线","2.00","2.00",""]
["工业网闸无线","3.00","0.00","属性：【wlgl_ww_zwym】【clgl_rkwg】【clgl_rkip】【clgl_ckwg】【clgl_ckip】，正确值：【255.255.255.0】【192.168.131.8】【192.168.132.6】【192.168.56.6】【192.168.56.5】，错误值：【255.255.255.192】【...】【192.168.131.8】【...】【192.168.56.6】"]
["斥候工业网关有线","3.00","3.00",""]
["云端配置页面网关维护","2.00","2.00",""]
["斥候工业网关无线","3.00","0.00","属性：【ippz_mm】【sbpz_ip】，正确值：【admin1234!】【192.168.129.5】，错误值：【admin1234！】【192.168.129.6】"]
["工业网闸有线","3.00","0.00","属性：【wlgl_ww_zwym】【clgl_rkwg】【clgl_rkip】【clgl_ckwg】【clgl_ckip】，正确值：【255.255.255.0】【192.168.80.6】【192.168.36.4】【192.168.49.6】【192.168.49.5】，错误值：【255.255.255.192】【】【】【】【】"]
["DB-IotLite网关无线","3.00","0.00","属性：【ippz_ip】【ippz_zwym】【cjdpz_jcqdz】【mqtt_qiyong】【mqtt_sssjfbzt】，正确值：【192.168.160.5】【255.255.255.192】【8193】【1】【dbzn/gateway/iotlite/2000808012】，错误值：【192.168.60.7】【255.255.255.0】【】【0】【dbzn/gateway/iotlite/网关SN号】"]
["DB-IotLite网关有线","4.00","0.00","属性：【ippz_ip】【ippz_zwym】【tdpz_qdmc】【tdpz_ip】【tdpz_port】【cjdpz_jcqdz】【mqtt_sssjfbzt】【mqtt_cjd_sbmc】【mqtt_cjd_tagid】，正确值：【192.168.64.3】【255.255.255.192】【ModbusTCPClient】【192.168.64.2】【502】【8195】【dbzn/gateway/iotlite/2000808010】【有线区精雕1】【MachinePamHID910】，错误值：【192.168.60.7】【255.255.255.0】【ModbusRTU_over_TCP】【192.168.60.7】【1883】【12514】【dbzn/gateway/iotlite/网关SN号】【】【】"]
["斥候工业网关有线","3.00","0.00","属性：【ippz_ip】【ippz_zwym】【sbpz_ip】【sbpz_port】【cjdpz_jcqdz】【mqtt_sssjfbzt】，正确值：【192.168.96.4】【255.255.255.192】【192.168.96.3】【502】【8210】【dbzn/gateway/iotlite/2000808011】，错误值：【192.168.60.7】【255.255.255.0】【192.168.60.7】【1883】【】【dbzn/gateway/iotlite/网关SN号】"]
["串口服务器无线","2.00","2.00",""]
["DB-IotLite网关有线","4.00","0.00","属性：【ippz_wangkou】【ippz_dns_sx】【tdpz_ip】【mqtt_sssjfbzt】，正确值：【ETH1】【223.5.5.5】【192.168.64.2】【dbzn/gateway/iotlite/2000808010】，错误值：【ETH0】【233.5.5.5】【192.168.64.3】【dbzn/gateway/iotlite/网关SN号】"]
["串口服务器有线","2.00","2.00",""]
["DB-IotLite网关无线","3.00","0.00","属性：【ippz_wifi_ssid】【wgpz_wgid】【tdpz_qdmc】【sbpz_sbid】【sbpz_sbmc】【sbpz_sbdz】【sbpz_jysb】【sbpz_jdzxz】【cjdpz_tagid】【cjdpz_mc】【cjdpz_sjq】【cjdpz_jcqdz】【cjdpz_cjsjlx】【cjdpz_zjx】【cjdpz_dxsx】【cjdpz_beilv】【mqtt_sssjfbzt】【mqtt_cjd_sbmc】【mqtt_cjd_tagid】，正确值：【无线区无线网】【WLAN-BOX1】【ModbusRTU_over_TCP】【无线区加工设备1】【无线区精雕1】【1】【0】【1】【MachinePamHID909】【急停状态】【4X (Holding Register)】【8193】【uint16】【Null】【只读】【1】【dbzn/gateway/iotlite/2000808012】【无线区精雕1】【MachinePamHID909】，错误值：【无限区无线网】【LAN-BOX1】【ModbusTCPClient】【】【】【】【】【】【】【】【】【】【】【】【】【】【dbzn/gateway/iotlite/网关SN号】【】【】"]
["斥候工业网关无线","3.00","0.00","属性：【wgpz_wgid】【sbpz_ip】【sbpz_port】【cjdpz_tagid】【mqtt_sssjfbzt】【mqtt_cjd_tagid】，正确值：【WLAN-BOX2】【192.168.129.5】【502】【MachinePamHID928】【dbzn/gateway/iotlite/2000808013】【MachinePamHID928】，错误值：【LAN-BOX2】【192.168.129.6】【1883】【MachinePamHID909】【dbzn/gateway/iotlite/网关SN号】【MachinePamHID909】"]
["工业网闸无线","3.00","0.00","属性：【wlgl_nw_name】【wlgl_nw_ip】【wlgl_ww_name】【wlgl_ww_ip】【dxgl】【clgl_name】【clgl_ydx】【clgl_mddx】【clgl_rkwg】【clgl_rkwk】【clgl_rkip】【clgl_ckwg】【clgl_ckwk】【clgl_ckip】【cmdlist_sbid】，正确值：【无线区网闸（内网）】【192.168.132.6】【无线区网闸（外网）】【192.168.56.5】【[{\"dx_name\":\"无线区路由器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.131.8\"},{\"dx_name\":\"数采服务器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.60.7\"}]】【无线区策略】【无线区路由器】【数采服务器】【192.168.131.8】【无线区网闸（内网）】【192.168.132.6】【192.168.56.6】【无线区网闸（外网）】【192.168.56.5】【无线区路由器命令】，错误值：【有线区网闸（内网）】【192.168.80.5】【有线区网闸（外网）】【192.168.49.5】【[{\"dx_name\":\"有线区交换机\",\"iplx\":\"IPV4\",\"ip\":\"192.168.66.4\"}]】【有线区策略】【有线区交换机】【有线区交换机】【192.168.80.6】【有线区网闸（内网）】【192.168.80.5】【192.168.49.6】【有线区网闸（外网）】【192.168.49.5】【有线区交换机命令】"]
["工业网闸有线","3.00","0.00","属性：【dxgl】【clgl_mddx】【clgl_rkip】【cmdlist_qsdz】【cmdlist_dzcd】【cmdlist_dz】，正确值：【[{\"dx_name\":\"有线区交换机\",\"iplx\":\"IPV4\",\"ip\":\"192.168.66.4\"},{\"dx_name\":\"数采服务器\",\"iplx\":\"IPV4\",\"ip\":\"192.168.60.7\"}]】【数采服务器】【192.168.36.4】【0】【65535】【允许】，错误值：【[{\"dx_name\":\"有线区交换机\",\"iplx\":\"IPV4\",\"ip\":\"192.168.66.4\"}]】【有线区交换机】【192.168.80.5】【】【】【】"]
["斥候工业网关有线","3.00","0.00","属性：【sbpz_ip】【cjdpz_tagid】【cjdpz_mc】【mqtt_sssjfbzt】【mqtt_cjd_tagid】，正确值：【192.168.96.3】【MachinePamHID917】【主轴转速】【dbzn/gateway/iotlite/2000808011】【MachinePamHID917】，错误值：【192.168.96.4】【MachinePamHID909】【急停状态】【dbzn/gateway/iotlite/网关SN号】【MachinePamHID909】"]
["斥候工业网关无线","3.00","0.00","属性：【cjdpz_tagid】【cjdpz_mc】【cjdpz_sjq】【cjdpz_jcqdz】【cjdpz_cjsjlx】【cjdpz_dxsx】【cjdpz_scms】【mqtt_cjd_tagid】，正确值：【MachinePamHID928】【切削速度】【4X (Holding Register)】【8227】【INT（16位有符号整数）】【只读】【Periodic】【MachinePamHID928】，错误值：【】【】【】【】【】【】【】【】"]
["云端配置页面网关维护","2.00","2.00",""]
["DB-IotLite网关有线","4.00","4.00",""]
["工业网闸有线","3.00","0.00","属性：【clgl_rkwg】【clgl_rkip】【clgl_ckwg】【clgl_ckip】，正确值：【192.168.80.6】【192.168.36.4】【192.168.49.6】【192.168.49.5】，错误值：【...】【192.168.80.6】【...】【192.168.49.6】"]
["串口服务器无线","2.00","2.00",""]
["工业网闸无线","3.00","0.00","属性：【clgl_ydx】【clgl_rkwg】【clgl_rkip】【clgl_ckwg】【clgl_ckip】，正确值：【无线区路由器】【192.168.131.8】【192.168.132.6】【192.168.56.6】【192.168.56.5】，错误值：【5200】【...】【192.168.131.8】【...】【192.168.56.6】"]
["DB-IotLite网关无线","3.00","0.00","属性：【ippz_wifi_mm】【ippz_dns_sx】，正确值：【admin1234!】【223.5.5.5】，错误值：【admin1234！】【23.5.5.5】"]
["斥候工业网关有线","3.00","3.00",""]
["云端配置页面网关配置","2.00","2.00",""]
["串口服务器有线","2.00","2.00",""]